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Loughrea Active Travel Scheme
Public Consultation – Non-statutory
Accessible Description of Existing and Proposed Visualisations 
There are four visualisations in total for this scheme. 
The ‘Existing’ and ‘Proposed’ visualisations include title-location to the top left of the page. Below on the left half side, there is an image of how the existing street/road looks like. On the right-hand side, there is an image of a photomontage of what the street/road is proposed to look like after the scheme is built. On top of these images, the subtitles read ‘EXISTING’ and ‘PROPOSED’ respectively.

Scheme Visualisation Danesfort 
This image was taken on Danesfort Road northbound (looking away from Loughrea town)  showing a view of Droim Na Cille  access junction.  

EXISTING
The image shows a view of the existing Danesfort Road at the entrance to Droim Na Cille estate and the existing zebra crossing with belisha beacons in the distance.  Zebra crossing is marked by black-and-white stripes and Belisha beacons – the black-and-white poles topped with flashing orange globes – and sits flat on the road surface, with footpath lowering to road level on both sides. 
There are footpaths either side of Danesfort Road and at the access to the estate. Buff colour skid resistance surfacing is shown on Danesfort Road on either approach to zebra crossing. White zig-zag lines are painted on the road on the approach to the crossing. Part of skid resistant surfacing and line marking have worn down. 
There are black bollards either side of pedestrian crossing. 
The footpath on the right turns sharply where it meets the side-road at the entrance to Droim Na Cille Estate. The entrance junction radii is generous, the junction is wide and there is dished kerb for pedestrians to cross.  

PROPOSED
The proposed image has been changed showing raised pedestrian crossing with ramps to slow traffic down on Danesfort. New belisha beacons with integrated lights are proposed to highlight the pedestrian crossing. Bollards are removed. The skid resistant surfacing and line marking is shown re-instated. 
Wider footpaths are shown on both sides of Danesfort. On the right, the image shows the footpath continue across the entrance to Droim Na Cille at a ramp with uncontrolled pedestrian crossing on top. 
The access junction is proposed to be narrowed to slow vehicles down on the entry and exit from the estate. 
The image shows cars approaching the pedestrian crossing on Danesfort while a pedestrian is crossin the road. pedestrians are shown on the footpaths either side of Danesfort Road. 

Scheme Visualisation Bohercom 
  
This image was taken on Bohercom looking towards the junction with Rockhaven on the right. 

EXISTING
The image shows a view of the existing Bohercom bounded with wide uneven verge and palisade fence to the left and old stone wall to the right. 
The stone wall terminates at the junction to Rockhaven. Footpath and houses with front gardens are shown to the right of Bohercom far side of Rockhaven junction. 
There is ‘Children crossing’ sign at the end of the palisade fence to the left and trees are shown to the left in the distance. 
There is existing One-way Road marking on Bohercom and Give-Way line at the Rockhaven junction giving priority to traffic in and out of Rockhaven. 
Bohercom carriageway is narrow, with narrow footpaths ahead. Public lighting columns are shown along the footpath. 
Image shows one car parked in the hard shoulder at the Rockhaven junction and one car parking over the footpath to the right, far side of the junction 

PROPOSED
The proposed image has been changed to show a raised table across the Rockhaven junction. Ramp marking is shown on the approach, and different colour surfacing is shown over the raised table. Kerbed rain garden is shown in the verge to the left. 
Double yellow road marking is shown around the bend at the entrance to Rockhaven to prevent parking at the junction.
Further up the street, the surface includes a cluster of painted coloured circles acts as school-zone markings, reinforcing the presence of the nearby school and highlighting the need for increased caution by drivers.

Scheme Visualisation Bride -GAA Club
  
This image was taken on Bride Street looking towards Loughrea town with GAA club wall on the right. Overhead utility wires run along timber poles on both sides, and a telecommunications mast is visible in the distance on the right

EXISTING
The image shows a wide and straight carriageway with cars parking either side of the street and very good forward visibility. The carriageway is wide with hard shoulders and uneven hard verge either side. There is a footpath in front of houses to the left. Hard surface is shown against the boundary wall of GAA club.
The carriageway has been recently resurfaced and is marked with white dashed centreline and yellow dashed edge line markings.
There is ponding in the hard strip to the left with cars parked between the footpath and the carriageway.  A van is parked against the tall boundary wall of the Loughrea GAA club on the right. 

PROPOSED
The proposed image has been changed to show that Bride Street has been narrowed, and parking bays have been provided on both sides. 
A raised zebra crossing  with beacons is shown across Bride Street. A footpath buildout is shown to the left, linking the new crossing with existing footpath in front of the houses. To the right, a two-way shared path for pedestrians and cyclists is shown adjacent to the Loughrea GAA wall. Footpath buildout is shown linking this shared path with the pedestrian crossing. 
Planted areas are shown on the GAA side of the new crossing.  


Scheme Visualisation Bride / Danesfort / Bohercom Junction

This image was taken on Bride Street looking towards Loughrea on the approach to Danesfort/Bohercom Junction. Shops, houses, and a church spire are visible in the distance, and mature trees overhang the footpath on the right.

EXISTING
The image shows a very wide and straight carriageway with footpaths and double yellow marking either side.
Several cars are visible in the distance. 
The junction ahead connects to side roads either side. There is a traffic signal-controlled pedestrian crossing on Bride Street far side of the junction. 

PROPOSED
The proposed image has been changed to show that Bride Street has been narrowed, footpath to the left has been widened and a two-way cycle track is proposed adjacent to the footpath on the right. 
Two cyclists travelling in opposite directions are shown on the cycle track. Person pushing a pram is shown on the footpath. Kerbs and planting buffer is shown separating the cycle track from the road and improving the appearance of the street.
Further ahead, the image shows a signalised junction with dedicated crossing facilities for pedestrians and cyclists. Toucan crossings are provided at the junction approaches, allowing pedestrians and cyclists to cross together at designated crossing points. Red tactile paving is provided at the crossings to help identify the crossing locations and improve accessibility.
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